PRILOG I DOKUMENTACIJE ZA NADMETANJE

PONUDBENI LIST/

ANNEX I OF TENDER DOCUMENTATION/

BID SHEET

Nabava opreme za opremanje strojnog pogona Bomark pak d.o.o / Supply of mechanical equipment of Bomark pak d.o.o

Naziv i broj Grupe nabave/ Name and Lot number: \_\_\_\_\_\_\_\_\_\_\_

Broj ponude/Offer number:\_\_\_\_\_\_\_ Datum ponude/ Offer date:\_\_\_\_\_\_\_\_\_

1. Naziv i sjedište Naručitelja/ Name and seat of the Contracting Authority

|  |  |
| --- | --- |
| Naručitelj/ Contracting Authority: | Bomak Pak d.o.o |
| Adresa/ Address: | Ivana Severa 15, 42 000 Varaždin, Hrvatska |
| OIB/ Identification/ Registration Number: | 86546227340 |

1. Naziv (tvrtka) i sjedište ponuditelja/ Name and seat of the tenderer

|  |  |
| --- | --- |
| Zajednica ponuditelja (zaokružiti)/ Lot o tenderers (circle) | DA/YES NE/NO |
| Ponuditelj/Tenderer: |  |
| Adresa/ Adress: |  |
| OIB (Identification / VAT number): |  |
| IBAN/ (bank account number): |  |
| Ponuditelj oslobođen PDV-a (zaokružiti)/ Tenderer is exempt from VAT (circle): | DA/YES NE/NO |
| Adresa za dostavu pošte/ Address for mail delivery: |  |
| Kontakt osoba ponuditelja/Contact person: |  |
| Telefon/Phone: |  |
| Faks/Fax: |  |
| E-pošta/E-mail: |  |

1. Cijena ponude/ Tender price

|  |  |
| --- | --- |
| Cijena ponude u HRK/EUR bez PDV-a/ Tender price in HRK or EUR net of VAT: |  |
| Iznos PDV-a/VAT : |  |
| Cijena ponude u HRK/EUR s PDV-om/ Tender price in HRK/EUR, VAT included: |  |

1. Rok valjanosti ponude/ Tender validity period

|  |  |
| --- | --- |
| Rok valjanosti ponude/ Tender validity period: |  |

Nakon što je proučio i razumio dokumentaciju za nadmetanje i sve uvjete nadmetanja, ponuditelj daje ponudu za jednu, više ili sve grupe nabave, čije su tehničke specifikacije opisane u Dodatku III Dokumentacije za nadmetanje, sve u skladu s odredbama Dokumentacije za nadmetanje./ After having read and understood the tender documents and all the conditions, the tenderer makes an offer for one, several or all lots of the procurement, whose technical specifications are described in Annex III of the Tender Documentation, all in accordance with the provisions of the Tender Documentation

\_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_/\_\_/20\_\_.

ZA PONUDITELJA/ ON BEHALF OF THE TENDERER:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(ime, prezime i potpis ovlaštene osobe/ name, signature of the authorised representative)

Ponudbeni list, PRILOG 1 - PODACI O ČLANOVIMA ZAJEDNICE PONUDITELJA *(priložiti/popuniti samo u slučaju zajedničke ponude)/* Bid Sheet, Annex 1, INFORMATION ABOUT THE MEMBERS OF CONSORTIA *(note: enclose only if the tender is group of tenderers/consortia[[1]](#footnote-1))*

1.Naziv (tvrtka) i sjedište člana zajednice ponuditelja/ Name and seat of the member of consortia 1)

|  |  |
| --- | --- |
| Član zajednice ponuditelja/ Member of consortia |  |
| Adresa/ Address: |  |
| OIB/ (Identification / VAT number): |  |
| IBAN/ (bank account number): |  |
| Ponuditelj oslobođen PDV-a/ (zaokružiti) Member is exempt from VAT(circle): | DA/YES NE/NO |
| Adresa za dostavu pošte/ Address for mail delivery:: |  |
| Kontakt osoba ponuditelja/ Contact person: |  |
| Telefon/ Phone: |  |
| Faks/ Fax: |  |
| E-pošta/ E-mail: |  |
| Dio ugovora koji će izvršavati član zajednice ponuditelja (navesti predmet, količinu, vrijednost i postotni dio)/ Part of the Contract to be executed by the member of consortia (subject, amount, value and percentage) : |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_/\_\_/20\_\_.

ZA ČLANA ZAJEDNICE PONUDITELJA/ ON BEHALF OF THE MEMBER OF CONSORTIA: :

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(ime, prezime i potpis ovlaštene osobe/ name, signature of the authorised representative)

Ponudbeni list; PRILOG 2 - PODACI O PODIZVODITELJIMA *(priložiti/popuniti samo u slučaju da se dio ugovora ustupa podizvoditeljima) /* Bid Sheet, Annex 1, INFORMATION ABOUT THE SUBCONTRACTORS *(note: enclose only if subcontractors are appointed[[2]](#footnote-2))*

1.Naziv (tvrtka) i sjedište podizvoditelja/ Name and seat of the subcontractor

|  |  |
| --- | --- |
| Subcontractor |  |
| Adresa/ Adress: |  |
| OIB/ (Identification / VAT number): |  |
| IBAN/(bank account number): |  |
| Podizvoditelj oslobođen od PDV-a (zaokružiti)/ Subcontractor is exempt from VAT: | DA/YES NE/NO |
| Kontakt osoba podizvoditelja/ Contact person: |  |
| Telefon/Phone: |  |
| Faks/Fax: |  |
| E-pošta/ E-mail: |  |
| Dio ugovora koji će izvršavati podizvoditelj (navesti predmet, količinu, vrijednost i postotni dio)/ Part of the Contract to be executed by the subcontractor (subject, amount, value and percentage): |  |

|  |  |
| --- | --- |
| Subcontractor |  |
| Adresa/ Adress: |  |
| OIB/ (Identification / registration number): |  |
| IBAN/(bank account number): |  |
| Podizvoditelj oslobođen od PDV-a (zaokružiti)/ Subcontractor is exempt from VAT: | DA/YES NE/NO |
| Kontakt osoba podizvoditelja/ Contact person: |  |
| Telefon/Phone: |  |
| Faks/Fax: |  |
| E-pošta/ E-mail: |  |
| Dio ugovora koji će izvršavati podizvoditelj (navesti predmet, količinu, vrijednost i postotni dio)/ Part of the Contract to be executed by the subcontractor (subject, amount, value and percentage): |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_/\_\_/20\_\_. ZA PONUDITELJA/ ON BEHALF OF TENDERER:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(ime, prezime i potpis ovlaštene osobe/ name and signature of authorised person)

PRILOG II DOKUMENTACIJE ZA NADMETANJE/ ANNEX II OF TENDER DOCUMENTATION

IZJAVA PONUDITELJA O NEPOSTOJANJU RAZLOGA ISKLJUČENJA/

STATEMENT REGARDING ABSENCE OF EXCLUSION CRITERIA

Nabava opreme za opremanje strojnog pogona Bomark pak d.o.o / Supply of mechanical equipment of Bomark pak d.o.o

Naziv i broj Grupe nabave/ Name and Lot number: \_\_\_\_\_\_\_\_\_\_\_

Radi dokazivanja nepostojanja situacija opisanih točkom 3.1. Dokumentacije za nadmetanje, a koje bi mogle dovesti do isključenja ponuditelja iz postupka javne nabave, dajem/For the purpose of proving the economic operator is not to be excluded from participation in this tender, I give the following

I Z J A V U/ S T A T E M E N T

kojom ja \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ iz \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (ime i prezime) (adresa stanovanja)

OIB:\_\_\_\_\_\_\_\_\_, broj osobne iskaznice \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ izdane od \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

kao po zakonu ovlaštena osoba za zastupanje gospodarskog subjekta

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(naziv i sjedište gospodarskog subjekta, OIB)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ pod materijalnom i kaznenom odgovornošću izjavljujem da /

I, \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ , from \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(name) (address) OIB/Identification/Registration

Number)

Number of identity card \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ issued from \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

as the authorised representative of the company

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(name and seat of the economic operator, OIB/ Identification/Registration Number)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

declare under penal and material responsibility:

1. ponuditelj niti osoba ovlaštena za zastupanje ponuditelja nisu pravomoćno osuđeni za bilo koje od sljedećih kaznenih djela odnosno za odgovarajuća kaznena djela prema propisima države sjedišta gospodarskog subjekta ili države čiji je državljanin osoba ovlaštena po zakonu za zastupanje gospodarskog subjekta/ The tenderer or the person authorised under the law to represent tenderer has not been convicted by final judgement for any of the following criminal acts or corresponding criminal acts under the legal provisions of the country in which the economic operator is established or of the country which a person authorised under the law to represent the economic operator is a citizen of:

a) prijevara (članak 236.), prijevara u gospodarskom poslovanju (članak 247.), primanje mita u gospodarskom poslovanju (članak 252.), davanje mita u gospodarskom poslovanju (članak 253.), zlouporaba u postupku javne nabave (članak 254.), utaja poreza ili carine (članak 256.), subvencijska prijevara (članak 258.), pranje novca (članak 265.), zlouporaba položaja i ovlasti (članak 291.), nezakonito pogodovanje (članak 292.), primanje mita (članak 293.), davanje mita (članak 294.), trgovanje utjecajem (članak 295.), davanje mita za trgovanje utjecajem (članak 296.), zločinačko udruženje (članak 328.) i počinjenje kaznenog djela u sastavu zločinačkog udruženja (članak 329.) iz Kaznenog zakona/ fraud (Article 236), fraudulent business activities (Article 247), accepting a bribe in business activities (Article 252), offering a bribe in business activities (Article 253), abuse in the public procurement procedure (Article 254), tax or customs duty evasion (Article 256), subsidy fraud (Article 258), money laundering (Article 265), abuse of position and powers (Article 291), illegal favouring (Article 292), accepting a bribe (Article 293), offering a bribe (Article 294), influence peddling (Article 295), influence peddling bribery (Article 296), criminal association (Article 328) and committing criminal act through criminal association (Article 329) under the

Criminal Code,

b)prijevara (članak 224.), pranje novca (članak 279.), prijevara u gospodarskom poslovanju (članak 293.), primanje mita u gospodarskom poslovanju (članak 294.a), davanje mita u gospodarskom poslovanju (članak 294.b), udruživanje za počinjenje kaznenih djela (članak 333.), zlouporaba položaja i ovlasti (članak 337.), zlouporaba obavljanja dužnosti državne vlasti (članak 338.), protuzakonito posredovanje (članak 343.), primanje mita (članak 347.) i davanje mita (članak 348.) iz Kaznenog zakona (»Narodne novine«, br. 110/97., 27/98., 50/00., 129/00., 51/01., 111/03., 190/03., 105/04., 84/05., 71/06., 110/07., 152/08., 57/11., 77/11. i 143/12.)/ fraud (Article 224), money laundering (Article 279), fraudulent business activities (Article 293), accepting a bribe in business activities (Article 294a), offering a bribe in business activities (Article 294b), association for committing criminal acts (Article 333), abuse of position and powers (Article 337), abuse of state power (Article 338), illegal mediation (Article 343), accepting a bribe (Article 347), and offering a bribe (Article 348) under the Criminal Code (Official Gazette 110/97, 27/98, 50/00, 129/00, 51/01, 111/03, 190/03, 105/04, 84/05, 71/06, 110/07, 152/08, 57/11, 77/11, and 143/12),

odnosno ponuditelj nije osuđen zbog svog profesionalnog ponašanje prema propisima države sjedišta gospodarskog subjekta/ and tenderer has not been convicted concerning their professional conduct, based on national legal provisions of the country of establishment .

1. ponuditelj je ispunio obvezu plaćanja dospjelih poreznih obveza i obveza za mirovinsko i zdravstveno osiguranje, osim ako mu prema posebnom zakonu plaćanje tih obveza nije dopušteno ili je odobrena odgoda plaćanja (primjerice u postupku predstečajne nagodbe)/ tenderer has not failed to fulfil the obligation to pay all outstanding tax liabilities and contributions for pension and health insurance, unless the economic operator was granted delayed payment of the said obligation under special regulations.

1. ponuditelj nije dostavio lažne podatke pri dostavi dokumenata koje je naručitelj naveo kao uvjet za sudjelovanje u postupku nabave/ tenderer has not submitted false information at the time of submitting documents on the basis of which it is determined whether or not the economic operator shall be excluded from participation

1. nad ponuditeljem nije otvoren stečaj, nije u postupku likvidacije, njime ne upravlja osoba postavljena od strane nadležnog suda, nije u nagodbi s vjerovnicima[[3]](#footnote-3), nije obustavio poslovne aktivnosti, nije predmetom sudskih postupaka zbog navedenih aktivnosti i nije u analognoj situaciji koja proizlazi iz sličnog postupka predviđenog nacionalnim zakonodavstvom ili propisima zemlje u kojoj ima poslovni nastan/ tenderer is not bankrupt, it is not being wound up or is in any stage of the bankruptcy proceeding, its affairs are not being administered by a person designated by the competent court, it has not entered into arrangement with creditors[[4]](#footnote-4),it has not suspended its business activities, or is not in a similar procedure under the national regulations of the country in which the tenderer is established.

te/and

1. ponuditelj nije u posljednje tri godine od dana početka postupka javne nabave učinio težak profesionalni propust odnosno nije kriv za neprofesionalno postupanje, a što Naručitelj može dokazati na bilo koji način/ tenderer has not committed grave professional misconduct in the previous three years up to the commencement of the public procurement procedure, which the Contracting Authority can prove by any means.

U \_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_/\_\_/20\_\_.

ZA PONUDITELJA/ ON BEHALF OF THE TENDERER : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(ime, prezime i potpis ovlaštene osobe/ name, signature of the authorised representative)

Samo za grupu 2 /Only for lot 2

PRILOG III DOKUMENTACIJE ZA NADMETANJE/ ANNEX III OF TENDER DOCUMENTATION

IZJAVA PONUDITELJA O DOSTAVI JAMSTVA/

STATEMENT ON DELIVERY OF PERFORMANCE GUARANTEE

Nabava opreme za opremanje strojnog pogona Bomark pak d.o.o / Supply of mechanical equipment of Bomark pak d.o.o

Naziv nabave/ Subject of procurement: \_\_\_\_\_\_\_\_\_\_\_

**IZJAVA O DOSTAVI JAMSTVA / STATEMENT ON DELIVERY OF PERFORMANCE GUARANTEE**

Za potrebe postupka Nabava opreme za opremanje strojnog pogona Bomark pak d.o. izjavljujemo da ćemo: / For the purposes of the procurement of Supply of mechanical equipment of Bomark pak d.o.o, we hereby irrevocalby declare that we will:

U roku od 10 (deset) kalendarskih dana od dana potpisivanja ugovora o robi Naručitelju predati jamstvo za uredno ispunjenje ugovora za slučaj povrede ugovornih obveza u obliku neopozive i bezuvjetne, bankarske garancije u korist Naručitelja, BOMARK PAK d.o.o., Ivana Severa 15, 42 000 Varaždin , OIB: 86546227340 i s klauzulom „plativo na prvi pisani poziv“ i „bez prigovora“, u iznosu od 5 % cijene naše ponude bez poreza na dodanu vrijednost s rokom valjanosti 120 dana od dana potpisa ugovora o robi uz respiro period od 60 (šezdeset) dana kojom se banka obvezuje platiti Naručitelju bilo koji iznos do visine iznosa koji pokriva bankarska garancija. /

Within ten (10) calendar days from the date of signing of the Contract, we will furnish to the Contracting Authority guarantee for the proper performance of the contract in case of breach of contractual obligations in the form of an irrevocable and unconditional, bank guarantees on behalf of contracting Authority - BOMARK PAK doo Ivana Severa 15, 42000 Varazdin OIB: 86546227340 with the clause "payable at first written call" and "no objection", in the amount of 5% of the price of our offer without value added tax valid for 120 days from the date of signing a supply contract with respiro period of 60 (sixty ), on which the bank agrees to pay the Contracting Authority any sums up to the amount covered by the bank guarantee.

U \_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_/\_\_/20\_\_.

ZA PONUDITELJA/ ON BEHALF OF THE TENDERER : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(ime, prezime i potpis ovlaštene osobe/ name, signature of the authorised representative)

PRILOG IV DOKUMENTACIJE ZA NADMETANJE

TEHNIČKE SPECIFIKACIJE/

ANNEX III OF TENDER DOCUMENTATION

TECHNICAL SPECIFICATIONS

Nabava opreme za opremanje strojnog pogona Bomark pak d.o.o / Supply of mechanical equipment of Bomark pak d.o.o

NAPOMENA/ NOTE :

Ponuditelj popunjava tehničke specifikacije samo za grupu nabave za koju daje ponudu, ili za više njih ukoliko daje ponudu za više grupa nabave./ Tenderer fills the technical specifications only for group for which it makes an offer, or for more groups if it is making an offer for more groups.

Ponuditelj obavezno popunjava stupac «Ponuđene karakteristike» definirajući detaljno tehničke specifikacije ponuđene robe (napomena: ponuditelj popunjava tehničke specifikacije upisujući točne karakteristike ponuđene robe, izbjegavajući pri tome popunjavanje stupca samo riječima kao što su npr. „zadovoljava“ , „DA“, „jednakovrijedno traženom“ ili „odgovara traženom“). Tenderer shall complete column „Specifications offered“, defining in detail technical specifications of offered supplies (note: tenderer fills the exact specifications of offered supplies, the words “compliant” and , “equivalent „or “yes” etc. are not sufficient).

Stupac « Bilješke, napomene, reference na dokumentaciju » ponuditelj može popuniti ukoliko smatra potrebnim. Stupac « Ocjena DA/NE » ponuditelj ne popunjava s obzirom na to da je stupac predviđen za ocjene Naručitelja./ Tenderer shall complete column „ Notes, remarks, references to documentation„ if it considers it necessary. Column „YES/NO“ is completed by the Contracting Authority.

Zahtjevi definirani Tehničkim specifikacijama predstavljaju minimalne tehničke karakteristike koje ponuđena roba mora zadovoljavati, ukoliko nije drugačije navedeno, te se iste ne smiju mijenjati od strane ponuditelja./ If not specified differently, Specifications Required are set out minimum technical requirements for the offered supplies and are not to be changed from the tenderer.

Grupa 1/ Lot 1 – Manipulatori-pneumatska ruka/Pneumatic arm manipulator

| **1**  **Item No. / *br. stavke*** | **2**  **Specifications Required /**  ***Tražene specifikacije*** | | **3**  **Specifications Offered /**  ***Ponuđene specifikacije*** | **4**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **5**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- | --- |
| **1.** | **Manipulator /** Manipulator  **Quantity /** količina**: 1** | |  | | |
|  | **Manufacturer’s name:** | |  | | |
|  | **Product type, model:** | |  | | |
| **1.1.** | **The platform** */* Platforma | **Min. Platform height 2000 mm** / Min. visina platforme 2000 mm |  |  |  |
| **1.2.** | **Handling Attachment** / Upravljačka ploča | **Specially adapted for automated capture of stretch film** / Specijalno prilagođen za automatizirano hvatanje stretch folije |  |  |  |
|  | **The possibility of rotation of 360 ° horizontally and vertically 90 °** / Mogućnost zakretanja od 360° horizontalno i vertikalno 90° |  |  |  |
|  | **Operated controls on arms control** / Upravlja se komandama na ručicama za upravljanje |  |  |  |
|  | **Pneumatic drive** / Pneumatski pogon |  |  |  |
|  | **Handle with integrated controls** / Ručica s integriranim komandama |  |  |  |
|  | **Min. load capacity 100 Kg** / Min. nosivost 100 Kg |  |  |  |
| **1.3.** | **Other features** / Ostale karakteristike | **Work radius from 500mm to 3500 mm /** Promjer radnog prostora od 500mm do 3500 mm |  |  |  |
|  | **Vertical lifting from 400 mm to 2000 mm** / Vertikalno dizanje od 400 mm do 2000 mm |  |  |  |
|  | **Degrees of freedom in all the joints +/- 360°** / Stupnjevi slobode u svim zglobovima +/- 360° |  |  |  |
|  | **Base plate for mounting max. dimension 700x700 mm** / Bazna ploča za montažu max. dimenzija 700x700 mm |  |  |  |
|  | **Fixing bolt min. M20 x 220 mm** / Vijci za fiksiranje min. M20 x 220mm |  |  |  |
|  | **Max. Laudness 70dBA** / Max. bučnost 70dBA |  |  |  |
|  | **Operation Temperature between 0°C - 45°C** / Radna temperature između **0°C - 45°C** |  |  |  |
|  | **Hydraulic power unit with electric motor max. 4kW /** Hidraulički agregat sa elektromotorom od max. 4kW |  |  |  |
| **1.4.** | **Delivery of equipment /** Isporuka opreme | **Max. 60 days /** Max. 60 dana |  |  |  |

**TECHNICAL SPECIFICATIONS – IMPLEMENTATION TASKS / *TEHNIČKE SPECIFIKACIJE – PROVEDBENI ZADACI***

| **I**  **Item no / *br. stavke*** | **II**  **Implementation tasks /*Provedbeni zadaci*** | **III**  **Specifications Offered (please specify the duration, resources and methodology proposed /**  ***Ponuđene specifikacije (molimo specificirajte trajanje, resurse i metodologiju)*** | **IV**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **V**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- |
| **1.** | **Testing at the premises of the buyer** / Testiranje na lokaciji kupca |  |  |  |
| **2.** | **Training for item 1 for 1 day; at least one week of delivery of equipment**  / Edukacija rada stroja u trajanju od 1 dana za stavku br. 1; najkasnije tjedan dana od isporuke opreme |  |  |  |

**TECHNICAL SPECIFICATIONS – AFTER-SALES SERVICES / *TEHNIČKE SPECIFIKACIJE - POST-PRODAJNE USLUGE***

| **I**  **Item no. / *Br. stavke*** | **II**  **After sales services / *Usluge*** | **III**  **Specifications Offered (please specify the duration, resources and methodology proposed /**  ***Ponuđene specifikacije (molimo specificirajte trajanje, resurse i metodologiju)*** | **IV**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **V**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- |
| 1. | **Standard min. 18 months warranty /** Standardno min. 18 mjeseci jamstvo |  |  |  |
| 2. | **Response time within 24 hours** / Odgovor na kvarove unutar 24 sata |  |  |  |

|  |  |  |
| --- | --- | --- |
| **Authorised contact person / *Ovlaštena kontakt osoba*** | | **Delivery address / *Adresa dostave*** |
| Name: | Juraj Vuksanić  Goran Kovačić | Bomark Pak d.o.o. production plant / Bomark pak d.o.o proizvodnja  Viktora Fizira 1, 42230 Ludbreg, Hrvatska |
| Phone: | +385 (0) 99 3120-599  +385 (0) 99 2563-928 |
| Fax: | +385 (0) 42 500 477 |
| E-mail: | g.kovacic@bomark.hr |
| Working hours: | 8 – 16 h local time |

Grupa 2/ Lot 2 - Električni viličar / Electric forklift

| **1**  **Item No. / *br. stavke*** | **2**  **Specifications Required /**  ***Tražene specifikacije*** | | **3**  **Specifications Offered /**  ***Ponuđene specifikacije*** | **4**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **5**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- | --- |
| **1.** | **Forklift**  **/** Viličar  **Quantity /** količina**: 2** | |  | | |
|  | **Manufacturer’s name:** | |  | | |
|  | **Product type, model:** | |  | | |
| 1.1. | ***System for lifting loads /*** sustav za dizanje tereta | **Crane triplex /** kran triplex |  |  |  |
|  | **Min. 2 cylinder in the middle** / min. 2 cilindra u sredini |  |  |  |
|  | **Min. 2 cylinder overside** / min. 2 cilindra bočno |  |  |  |
|  | **Uniform stabilization at lifting** / ravnomjerna stabilizacija kod podizanja tereta |  |  |  |
|  | **Minimum lifting height 4700 mm** / minimalna visina dizanja 4700 mm |  |  |  |
|  | **Max. Free travel 1650mm** /Max. Slobodan hod 1650mm |  |  |  |
|  | **Minimum load capacity of 2000 kg /** minimalna nosivost terete 2000 kg |  |  |  |
| 1.2. | ***Motor for driving /*** *motor za vožnju* | **Min. 2 pcs AC motor technology /** min. 2 kom motora AC tehnologija |  |  |  |
|  | **Power of motor min. 4.7 kW /** snaga motora min. 4,7 kW |  |  |  |
|  | **Min. speed 15 km / h /** min. brzina vožnje 15 km/h |  |  |  |
| 1.3. | ***Engine for lift loads /*** *motor za podizanje tereta* | **Min. motor power 14 kW /** min. snaga motora 14 kW |  |  |  |
|  | **Low-noise pump /** niska razina buke pumpe |  |  |  |
|  | **Min. lifting speed with load 410 mm / s /** min. brzina podizanja s teretom 410 mm/s |  |  |  |
|  | **Min. lifting speed without load 600 mm /** **s** / min. brzina podizanja bez tereta 600 mm/s |  |  |  |
| 1.4. | ***Battery /*** *baterija* | **Min. 2 pieces /** min. 2 komada |  |  |  |
|  | **48 V /** 48 V |  |  |  |
|  | **Min. 750 Ah /** min. 750 Ah |  |  |  |
|  | **Locking device battery** / uređaj za zaključavanje baterije |  |  |  |
|  | **Lateral replacement battery** / bočna izmjena baterije |  |  |  |
|  | **Min. 1 trolley for a quick change of battery** / min. 1 kolica za brzu izmjenu baterije |  |  |  |
|  | **With a system for topping up water /** Sa sustavom za nadolijevanje vode |  |  |  |
| 1.5. | ***Battery Charger /*** *Punjač za baterije* | **48 V /** 48 V |  |  |  |
|  | **Max. 8 hours charge time batteries /** max. 8 sati trajanje punjenja baterije |  |  |  |
| 1.6. | ***Display /*** *displej* | **LCD /** LCD |  |  |  |
|  | **The ability to provide quick selection of travel /** mogućnost pružanja brzog odabira vožnje |  |  |  |
|  | **Display speed limits /** prikaz brzine vožnje |  |  |  |
|  | **Display of additional loads /** prikaz dodatnih opterećenja |  |  |  |
|  | **Display battery status /** prikaz stanja baterije |  |  |  |
|  | **Display with self-diagnostic** / Prikaz sa samodijagnostikom |  |  |  |
| 1.7. | ***OPPS system /*** *OPPS sustav* | **Security drive system /** sigurnosni sustav vožnje |  |  |  |
| 1.8. | ***Other equipment /*** *ostala oprema* | **Min. 4 valves /** min. 4 ventila |  |  |  |
|  | **LED taillights** / LED stražnja svjetla |  |  |  |
|  | **Rearview mirror /** retrovizor |  |  |  |
|  | **Integrated lateral shift /** Integrirani bočni pomak |  |  |  |
|  | **Fork min. 1200 mm /** Vilice min. 1200 mm |  |  |  |
|  | **Full rubber SE /** Gume pune SE |  |  |  |
|  | **Min. 2 lines on the fork carriage /** min. 2 linija na kolicima vilica |  |  |  |
|  | **Max. 3 wheels** / Max. 3 kotača |  |  |  |
|  | **Beep reversing /** Zvučni signal vožnje unazad |  |  |  |
| 1.9. | ***Cabin /*** *Kabina* | **Steel closed cabin /** Čelična zatvorena kabina |  |  |  |
|  | **Heating and cooling cabins /** Grijanje i hlađenje kabine |  |  |  |
| 1.10. | ***Forklift Dimensions /*** Dimenzije viličara | **Max. height forklifts 2150mm /** Max. visina viličara 2150 mm |  |  |  |
|  | **Max. length forklift 2010 mm /** Max. dužina viličara 2010 mm |  |  |  |
|  | **Max. width forklift 1110 mm /** Max. širina viličara 1110 mm |  |  |  |
|  | **Max. weight forklift 3650 Kg** / Max. težina viličara 3650 kg |  |  |  |
| 1.11. | ***Delivery of equipment /*** *Isporuka opreme* | **Max. 4 months /** Max. 4 mjeseca |  |  |  |

**TECHNICAL SPECIFICATIONS – IMPLEMENTATION TASKS / *TEHNIČKE SPECIFIKACIJE – PROVEDBENI ZADACI***

| **I**  **Item no / *br. stavke*** | **II**  **Implementation tasks /*Provedbeni zadaci*** | **III**  **Specifications Offered (please specify the duration, resources and methodology proposed /**  ***Ponuđene specifikacije (molimo specificirajte trajanje, resurse i metodologiju)*** | **IV**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **V**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- |
| **1.** | **Testing at the premises of the buyer** / Testiranje na lokaciji kupca |  |  |  |
| **2.** | **Training for item 1 for 1 day; at least one week of delivery of equipment**  / Edukacija rada stroja u trajanju od 1 dana za stavku br. 1; najkasnije tjedan dana od isporuke opreme |  |  |  |

**TECHNICAL SPECIFICATIONS – AFTER-SALES SERVICES / *TEHNIČKE SPECIFIKACIJE - POST-PRODAJNE USLUGE***

| **I**  **Item no. / *Br. stavke*** | **II**  **After sales services / *Usluge*** | **III**  **Specifications Offered (please specify the duration, resources and methodology proposed /**  ***Ponuđene specifikacije (molimo specificirajte trajanje, resurse i metodologiju)*** | **IV**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **V**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- |
| 1. | **Standard 2 year warranty or 4000 working hours** Dvogodišnje jamstvo ili 4000 radnih sati |  |  |  |
| 2. | **Response time within 24 hours** / Odgovor na kvarove unutar 24 sata |  |  |  |

|  |  |  |
| --- | --- | --- |
| **Authorised contact person / *Ovlaštena kontakt osoba*** | | **Delivery address / *Adresa dostave*** |
| Name: | Juraj Vuksanić  Goran Kovačić | Bomark Pak d.o.o. production plant / Bomark pak d.o.o proizvodnja  Viktora Fizira 1, 42230 Ludbreg, Hrvatska |
| Phone: | +385 (0) 99 3120-599  +385 (0) 99 2563-928 |
| Fax: | +385 (0) 42 500 477 |
| E-mail: | g.kovacic@bomark.hr |
| Working hours: | 8 – 16 h local time |

Grupa 3/ Lot 3 - Platform digital scale / Platformska digitalna vaga

| **1**  **Item No. / *br. stavke*** | **2**  **Specifications Required /**  ***Tražene specifikacije*** | | **3**  **Specifications Offered /**  ***Ponuđene specifikacije*** | **4**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **5**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- | --- |
| **1.** | **Platform digital scale**  **/** Platformska digitalna vaga  **Quantity /** količina**: 1** | |  | | |
|  | **Manufacturer’s name:** | |  | | |
|  | **Product type, model:** | |  | | |
| **1.1.** | ***Platform scales /*** Platforma vage | **Width between 1300mm to 1600mm /** Širina između 1300mm do 1600mm |  |  |  |
|  | **Length between 1300mm to 1600mm** / Dužina između 1300mm do 1600mm |  |  |  |
|  | **Fully painted platform** / Bojana platforma |  |  |  |
|  | **Min. 4 load cells of min. 2000 Kg measuring range** / Min. 4 mjerne ćelije od min. 2000 Kg mjernog raspona |  |  |  |
| **1.2.** | **Display panel** / Pokazni uređaj | **RS232 or equvalent** / RS232 ili jednakovrijedan |  |  |  |
|  | **Digit size from 20mm to 30mm** / Veličina znamenki od 20mm do 30mm |  |  |  |
|  | **LCD with white LED backlight** / LCD s bijelim LED pozadinskim osvjetljenjem |  |  |  |
|  | **Between 5 to 10 keys /** Između 5 do 10 tipki |  |  |  |
|  | **ABS plastic case or equivalent /** ABS plastično kučište ili jednakovrijedno |  |  |  |
|  | **Rechargeable batteries min. 6V/4Ah /** Punjive baterije min. 6V/4Ah |  |  |  |
|  | **AC adapter to charge the battery (min. 12V / 500mA)**/ AC adapter za punjenje baterija (min. 12V/500mA) |  |  |  |
|  |  | **The certified by the DZM-a or authorized organization /** Ovjereno od strane DZM-a ili ovlaštenog tijela |  |  |  |
| 1.3. | **Ramp** / Navoz | **Ramp for the possibility of importing goods with a manual forklift /** Rampa za mogućnost navoza robe ručnim viličarem |  |  |  |
| 1.4. | **Delivery of equipment /** Isporuka opreme | **Max. 2 weeks /** Max. 2 tjedna |  |  |  |

Grupa 4/ Lot 4 – Stroj za ovijanje paleta / Machine for wrapping pallets

| **1**  **Item No. / *br. stavke*** | **2**  **Specifications Required /**  ***Tražene specifikacije*** | | **3**  **Specifications Offered /**  ***Ponuđene specifikacije*** | **4**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **5**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- | --- |
| **1.** | **Machine for wrapping pallets /** Stroj za ovijanje paleta  **Quantity /** količina**: 1** | |  | | |
|  | **Manufacturer’s name:** | |  | | |
|  | **Product type, model:** | |  | | |
| **1.1.** | **The platform of the machine for wrapping pallets**  */* Platforma stroja za ovijanje paleta | **Variable Preestretch in the range of 150% to 400%** / Promjenjivo prednatezanje u rasponu od 150% do 400% |  |  |  |
|  | **Min. two independent drive motor** / Min. dva neovisna pogonska motora |  |  |  |
|  | **Diameter of rotary platform min. 1600mm** / Promjer rotacijske platforme min. 1600mm |  |  |  |
|  | **Turning platform with selectable speeds ranging from min. 4 rpm to max. 12 rpm** / Okretanje platforme sa mogučnošću odabira brzine u rasponu od min.4 o/min do max. 12 o/min |  |  |  |
|  | **Chain transfer method or equal value** / Lančani način prijenosa ili jednako vrijedno |  |  |  |
|  | **Max. Platform height with rotate plate 80mm** / Max. visina platforme sa okretnom pločom 80mm |  |  |  |
|  | **Min. Tower height 3100 mm** / Min. visina stupa 3100 mm |  |  |  |
|  | **Wrapping height of 100 mm to 2800 mm** / Visina ovijanja od 100 mm do 2800 mm |  |  |  |
|  | **Power supply 230V; 1 phase; 50 Hz** / Napajanje 230V; 1 faza; 50 Hz |  |  |  |
|  | **Max. installed capacity of 2.2 kW** / Max. instalirana snaga 2,2 kW |  |  |  |
|  | **Min. platform capacity 2000 Kg** / Min. nosivost platforme 2000 Kg |  |  |  |
|  | **Possibility of max. outside diameter 300 mm foil** / Mogućnost prihvata max. vanjskog promjera folije 300 mm |  |  |  |
|  | **Possibility of max. width film 500 mm** / Mogućnost prihvata max. širine folije 500 mm |  |  |  |
|  | **Possibility of wrapping foil thickness in the range of 17 - 35my** / Mogućnost omatanja folijom debljine u rasponu od 17 – 35my |  |  |  |
|  | **Acceptance of the inner diameter of the sleeve 76mm** / Prihvat unutarnjeg promjera tuljka 76mm |  |  |  |
|  | **Acceptance min. weight sheet of 20 Kg** / Prihvat min. težine folije od 20 Kg |  |  |  |
| **1.2.** | **Multilevel controling** / Kontrola na više razina | **Possibility to set different parameters of wrapping: at the bottom of the pallets, in the middle going upwards, on the upper part of pallet, in the middle of the pallet going down, and in the end of wrapping at the bottom of the pallets** / Mogućnost podešavanja različitih parametara ovijanja na dnu palete, na sredini prema gore, gornjem dijelu, u sredini prilikom spuštanja, i na kraju ovijanja pri dnu palete |  |  |  |
|  | **Min. wrapping at 9 level**  / Min. ovijanje na 9 nivoa |  |  |  |
| **1.3.** | **Other features** / Ostale karakteristike | **Slow start and stop** / Polagano pokretanje i zaustavljanje |  |  |  |
|  |  | **Stopping at the same place** / Zaustavljanje na istom mjestu |  |  |  |
|  |  | **Automatic determination a range of height** **pallets** / Automatsko određivanje visine palete |  |  |  |
|  |  | **Choosing the cycle of wrapping up and down or just up or just down** / Biranje ciklusa ovijanja gore-dolje ili samo gore ili samo dolje |  |  |  |
|  |  | **Adjust the volume of preestretch and stretch from the control panel** / Reguliranje jačine prednatezanja i zatezanja folije preko upravljačke ploče |  |  |  |
|  |  | **Regulating the number of wrapping at the bottom and at the top of the pallet** / Reguliranje broja ovijanja na dnu i na vrhu palete |  |  |  |
|  |  | **Regulating speed** **of platform**/ Reguliranje brzine okretanja platforme |  |  |  |
|  |  | **Regulating the speed of the carrier foil** / Reguliranje brzine nosača folije |  |  |  |
|  |  | **Regulating delay photocell / off photocell** / Reguliranje kašnjenja fotoćelije/isključivanje fotoćelije |  |  |  |
|  |  | **Program for insert cover sheets** / Program za umetanje prekrivne folije |  |  |  |
|  |  | **Start wrapping from the reference level** / Start ovijanja od zadane visine |  |  |  |
|  |  | **The possibility of manual adjustment stretch foil** / Mogućnost ručnog podešavanja zatezanja folije |  |  |  |
|  |  | **Optional pressure plate** / Opcija potisne ploče |  |  |  |
|  |  | **Programming, recording and playback min. 12 wrapping programs** / Programiranje, snimanje i reproduciranje min. 12 programa ovijanja |  |  |  |
| **1.4.** | **Delivery of equipment /** Isporuka opreme | **Max. 5 weeks /** Max. 5 tjedna |  |  |  |

**TECHNICAL SPECIFICATIONS – IMPLEMENTATION TASKS / *TEHNIČKE SPECIFIKACIJE – PROVEDBENI ZADACI***

| **I**  **Item no / *br. stavke*** | **II**  **Implementation tasks /*Provedbeni zadaci*** | **III**  **Specifications Offered (please specify the duration, resources and methodology proposed /**  ***Ponuđene specifikacije (molimo specificirajte trajanje, resurse i metodologiju)*** | **IV**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **V**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- |
| **1.** | **Testing at the premises of the buyer** / Testiranje na lokaciji kupca |  |  |  |
| **2.** | **Training for item 1 for 1 day; at least one week of delivery of equipment**  / Edukacija rada stroja u trajanju od 1 dana za stavku br. 1; najkasnije tjedan dana od isporuke opreme |  |  |  |

**TECHNICAL SPECIFICATIONS – AFTER-SALES SERVICES / *TEHNIČKE SPECIFIKACIJE - POST-PRODAJNE USLUGE***

| **I**  **Item no. / *Br. stavke*** | **II**  **After sales services / *Usluge*** | **III**  **Specifications Offered (please specify the duration, resources and methodology proposed /**  ***Ponuđene specifikacije (molimo specificirajte trajanje, resurse i metodologiju)*** | **IV**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **V**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- |
| 1. | **Standard min. 18 months warranty /** Standardno min. 18 mjeseci jamstvo |  |  |  |
| 2. | **Response time within 24 hours** / Odgovor na kvarove unutar 24 sata |  |  |  |

|  |  |  |
| --- | --- | --- |
| **Authorised contact person / *Ovlaštena kontakt osoba*** | | **Delivery address / *Adresa dostave*** |
| Name: | Juraj Vuksanić  Goran Kovačić | Bomark Pak d.o.o. production plant / Bomark pak d.o.o proizvodnja  Viktora Fizira 1, 42230 Ludbreg, Hrvatska |
| Phone: | +385 (0) 99 3120-599  +385 (0) 99 2563-928 |
| Fax: | +385 (0) 42 500 477 |
| E-mail: | g.kovacic@bomark.hr |
| Working hours: | 8 – 16 h local time |

Grupa 5/ Lot 5 – Prijenosno računalo sa operativnim sustavom /The laptop with operating system

| **1**  **Item No. / *br. stavke*** | **2**  **Specifications Required /**  ***Tražene specifikacije*** | | **3**  **Specifications Offered /**  ***Ponuđene specifikacije*** | **4**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **5**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- | --- |
| **1.** | **Laptop**  **/** Prijenosno računalo  **Quantity /** količina**: 2** | |  | | |
|  | **Manufacturer’s name:** | |  | | |
|  | **Product type, model:** | |  | | |
| **1.1.** | ***Basic features /*** Osnovne karakteristike | **CPU brand Intel or equivalent /** CPU Intel ili jednakovrijedan |  |  |  |
|  | **CPU type Core i5 or equivalent** / CPU tip Core i5 ili jednakovrijedan |  |  |  |
|  | **Min. CPU speed of 2.50 GHz** / Min. CPU brzina 2,50 GHz |  |  |  |
|  | **Min. Core 2** / Min. Core 2 |  |  |  |
|  | **L3 Cashe min. 3 MB** / L3 Cashe min. 3 MB |  |  |  |
|  | **Chipset integrated with processor** / Chipset integriran s procesorom |  |  |  |
|  | **Memory min. 4 GB** / Memorija min. 4 GB |  |  |  |
|  | **Min. Memory Clock Speed 2133 MHz /** Min. takt memorije 2133 MHz |  |  |  |
|  | **Memory slot DIMM DDR4 or equivalent /** Memorijski utor SO-DIMM DDR4 ili jednakovrijedan |  |  |  |
|  | **Min. 2 memory slots** / Min. 2 memorijska utora |  |  |  |
|  | **Screen min. 15,6” /** Ekran min. 15,6” |  |  |  |
|  | **Display Type AG (Anti-Glare) or equivalent /** Vrsta zaslona AG (AntiGlare) ili jednakovrijedan |  |  |  |
|  | **Min. resolution 1366x768** / Min. rezolucija 1366x768 |  |  |  |  |  |
|  | **HDD SATA or equivalent** / HDD SATA 500 ili jednakovrijedan |  |  |  |
|  | **RPM HDD min. 7,200 rpm** / Broj okretaja HDD-a min. 7.200 rpm |  |  |  |
| 1.2. | **Other features** / Ostale karakteristike | **Operating System min. Windows 10** / Operativni sustav min. Windows 10 |  |  |  |
|  | **VGA: Intel HD or equivalent** / VGA: Intel HD ili jednakovrijedan |  |  |  |
|  | **Optical drive DVD +/- RW** **DL** / Optička jedinica DVD+/-RW DL |  |  |  |
|  | **Audio: HD audio with DTS Studio Sound, integrated stereo speakers, dual-microphone array /** Audio: HD Audio sa DTS Studio Sound, integrirani stereo zvučnici, dual-mikrofon |  |  |  |
|  | **Network 802.11ac /** Mreža 802.11 ac |  |  |  |
|  | **Video camera HD 720p /** Video kamera HD 720p |  |  |  |
|  | **The card reader SD** / Čitač kartica SD |  |  |  |
| 1.3. | **Rear panel** / Stražnji panel | **HDMI min. 1 pcs /** HDMI min. 1 kom |  |  |  |
|  | **Audio In/Out min. 1 pcs /** Audio Ulaz/Izlaz min. 1 kom |  |  |  |
|  | **USB 2.0 min. 2 pcs /** USB 2.0 min. 2 kom |  |  |  |
|  | **USB 3.0 min. 1 pcs /** USB 3.0 min. 1 kom |  |  |  |
|  | **USB 3.1 min. 1 pcs /** USB 3.1 min. 1 kom |  |  |  |
| 1.4. | **Dimensions and weight /** Dimenzije i masa | **Max. weight 2.5 Kg** / Max. težina 2,5 Kg |  |  |  |
|  | **Li-Ion 3-cell or equivalent** / Baterija Li-Ion 3 ćelije ili jednakovrijedan |  |  |  |
|  | **The keyboard spill-resistant** / Tipkovnica otporna na prolijevanje tekućine |  |  |  |
| 1.5. | ***Delivery of equipment /*** *Isporuka opreme* | **Max. 4 weeks /** Max. 4 tjedna |  |  |  |

**TECHNICAL SPECIFICATIONS – IMPLEMENTATION TASKS / *TEHNIČKE SPECIFIKACIJE – PROVEDBENI ZADACI***

| **I**  **Item no / *br. stavke*** | **II**  **Implementation tasks /*Provedbeni zadaci*** | **III**  **Specifications Offered (please specify the duration, resources and methodology proposed /**  ***Ponuđene specifikacije (molimo specificirajte trajanje, resurse i metodologiju)*** | **IV**  **Notes, remarks,  ref to documentation /**  ***Bilješke, napomene, reference na dokumentaciju*** | **V**  **Evaluation Committee’s notes /**  ***Bilješke evaluacijskog odbora*** |
| --- | --- | --- | --- | --- |
| **1.** | **Testing at the premises of the buyer** / Testiranje na lokaciji kupca |  |  |  |
| **2.** | **Training for item 1 for 1 day; at least one week of delivery of equipment**  / Edukacija rada stroja u trajanju od 1 dana za stavku br. 1; najkasnije tjedan dana od isporuke opreme |  |  |  |

PRILOG IV DOKUMENTACIJE ZA NADMETANJE

FINANCIJSKA PONUDA/

ANNEX IV OF TENDER DOCUMENTATION

FINANCIAL OFFER

Nabava opreme za opremanje strojnog pogona Bomark pak d.o.o / Supply of mechanical equipment of Bomark pak d.o.o

Grupa 1/ Lot 1 – Manipulatori-pneumatska ruka / Pneumatic arm manipulator

Grupa 2/ Lot 2 – Električni viličar / Electric forklift

Grupa 3/ Lot 3 - Platformska diditalna vaga / Platform digital scale

Grupa 4/ Lot 4 – Stroj za ovijanje paleta / Machine for wrapping pallets

Grupa 5/ Lot 5 – Prijenosno računalo sa operativnim sustavom / The laptop with operating system

TROŠKOVNIK/ FINANCIAL OFFER

za Grupu 1/ for Lot 1: Manipulatori-pneumatska ruka / Pneumatic arm manipulator

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Predmet br./ Item | Predmet nabave/ Subject of procurement | Jedinica mjere/ Unit | Količina/ Quantity | Jedinična cijena u HRK/EUR (bez PDV-a)/ Unit price in HRK/EUR net of VAT | Ukupna cijena uHRK/EUR (bez  PDV-a)/ Total price in HRK/EUR net of VAT |
| 1. | Manipulatori-pneumatska ruka / Pneumatic arm manipulator | Komplet/Set | 1 |  |  |
|  | | | |  |  |
| Cijena ponude u HRK/EUR bez poreza na dodanu vrijednost/ Total price in HRK/EUR net of VAT | | | |  |  |
| Iznos poreza na dodanu vrijednost/ VAT: | | | |  |  |
| Cijena ponude u HRK/EUR s porezom na dodanu vrijednost / Total price in HRK/EUR, VAT included: | | | |  |  |

FINANCIJSKA PONUDA/ FINANCIAL OFFER

za Grupu 2/ for Lot 2 – Električni viličar / Electric forklift

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Predmet br./ Item | Predmet nabave/ Subject of procurement | Jedinica mjere/ Unit | Količina/ Quantity | Jedinična cijena u HRK/EUR (bez PDV-a)/ Unit price in HRK/EUR net of VAT | Ukupna cijena u HRK/EUR (bez  PDV-a)/ Total price in HRK/EUR net of VAT |
| 1. | Električni viličar / Electric forklift | Komplet/Set | 2 |  |  |
|  | | | |  |  |
| Cijena ponude u HRK/EUR bez poreza na dodanu vrijednost/ Total price in HRK/EUR net of VAT | | | |  |  |
| Iznos poreza na dodanu vrijednost/ VAT: | | | |  |  |
| Cijena ponude u HRK/EUR s porezom na dodanu vrijednost / Total price in HRK/EUR, VAT included: | | | |  |  |

FINANCIJSKA PONUDA/ FINANCIAL OFFER

za Grupu 3/ for Lot 3 – Platformska diditalna vaga / Platform digital scale

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Predmet br./ Item | Predmet nabave/ Subject of procurement | Jedinica mjere/ Unit | Količina/ Quantity | Jedinična cijena u HRK/EUR (bez PDV-a)/ Unit price in HRK/EUR net of VAT | Ukupna cijena u HRK/EUR (bez  PDV-a)/ Total price in HRK/EUR net of VAT |
| 1. | Platformska diditalna vaga / Platform digital scale | Komplet/Set | 1 |  |  |
|  | | | |  |  |
| Cijena ponude u HRK/EUR bez poreza na dodanu vrijednost/ Total price in HRK/EUR net of VAT | | | |  |  |
| Iznos poreza na dodanu vrijednost/ VAT: | | | |  |  |
| Cijena ponude u HRK/EUR s porezom na dodanu vrijednost / Total price in HRK/EUR, VAT included: | | | |  |  |

FINANCIJSKA PONUDA / FINANCIAL OFFER

za Grupu 4/ for Lot 4 – Stroj za ovijanje paleta / Machine for wrapping pallets

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Predmet br./ Item | Predmet nabave/ Subject of procurement | Jedinica mjere/ Unit | Količina/ Quantity | Jedinična cijena u HRK/EUR (bez PDV-a)/ Unit price in HRK/EUR net of VAT | Ukupna cijena u HRK/EUR (bez  PDV-a)/ Total price in HRK/EUR net of VAT |
| 1. | Stroj za ovijanje paleta / Machine for wrapping pallets | Komplet/Set | 1 |  |  |
|  | | | |  |  |
| Cijena ponude u HRK/EUR bez poreza na dodanu vrijednost/ Total price in HRK/EUR net of VAT | | | |  |  |
| Iznos poreza na dodanu vrijednost/ VAT: | | | |  |  |
| Cijena ponude u HRK/EUR s porezom na dodanu vrijednost / Total price in HRK/EUR, VAT included: | | | |  |  |

FINANCIJSKA PONUDA / FINANCIAL OFFER

za Grupu 5/ for Lot 5 – Prijenosno računalo sa operativnim sustavom / The laptop with operating system

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Predmet br./ Item | Predmet nabave/ Subject of procurement | Jedinica mjere/ Unit | Količina/ Quantity | Jedinična cijena u HRK/EUR (bez PDV-a)/ Unit price in HRK/EUR net of VAT | Ukupna cijena u HRK/EUR (bez  PDV-a)/ Total price in HRK/EUR net of VAT |
| 1. | Prijenosno računalo sa operativnim sustavom / The laptop with operating system | Komplet/Set | 2 |  |  |
|  | | | |  |  |
| Cijena ponude u HRK/EUR bez poreza na dodanu vrijednost/ Total price in HRK/EUR net of VAT | | | |  |  |
| Iznos poreza na dodanu vrijednost/ VAT: | | | |  |  |
| Cijena ponude u HRK/EUR s porezom na dodanu vrijednost / Total price in HRK/EUR, VAT included: | | | |  |  |

1. Ispuniti za svakog člana zajednice ponuditelja zasebno/ To be submitted for each member of consortia seperatly [↑](#footnote-ref-1)
2. Ispuniti za svakog podizvoditelja zasebno/ To be submitted for subcontractor separately

   [↑](#footnote-ref-2)
3. Sklopljena predstečajna nagodba ne predstavlja nagodbu s vjerovnicima za potrebe ove dokumentacije [↑](#footnote-ref-3)
4. Pre-bankruptcy settlement does not represent the arrangement with creditors within the meaning of this documentation [↑](#footnote-ref-4)